# Low-Level Design — NewCo

## Pod Topology

### Pod 1

* Site: DC1 (Central US)
* UAG: internet-facing × 2
* vCenter: vcsa01.newco.com ### Pod 2
* Site: DC2 (US East 2)
* UAG: internet-facing × 2
* vCenter: vcsa02.newco.com

## Image Build

* Base OS: Windows 11 23H2
* Instant Clone: Yes
* DEM: Yes
* FSLogix: Yes

## Network, DNS, NTP

* Provided by customer; specifics to be captured during implementation.

## Assumptions & Dependencies

* DNS/NTP/routing provided by customer